RAKOv

1. Zrihtamo internet

V cmd napišemo **ipconfig**

A computer screen shot of a computer

AI-generated content may be incorrect.

In razberemo ip od nšga primarnega vmesnika torej Ethernet 2(na testu bo vrjetno samo Ethernet) in napišemo default gateway v brskalnik v mojem primeru **192.168.1.1**

Pršli bomo na neki tazga

A screenshot of a computer

AI-generated content may be incorrect.

In v zgornem desnem kotu kliknemo **Quick Set**

Vrže ns na neki temu podobnega

A screenshot of a computer

AI-generated content may be incorrect.

Tole bo nastavlen na automatic spremeni na static

A screenshot of a computer

AI-generated content may be incorrect.

A screenshot of a computer

AI-generated content may be incorrect.

Ko mamo napišemo not podatke iz listka

A close up of a paper

AI-generated content may be incorrect.

Zgled:

A screenshot of a computer

AI-generated content may be incorrect.

Zdej nm internet dela supr!

Ps. Treba je odklopt kabl povezan na main net tko da lahko ga vm potegneš al pa greš v control panel od windowsa pa pod omrežje in tm ugansneš umesnik

(sam kabl vm povleč)

1. Spremenimo Vmesnik  
   Postopek dostopa do omrežnih nastavitev
   1. Kliknemo gumb nastavitve  
      A screenshot of a computer

      AI-generated content may be incorrect.
   2. Gremo pod zavihek omrežje

**A screenshot of a computer

AI-generated content may be incorrect.**

Po defaultu je nastavlen Vnesnik v VM-ju tko

A screenshot of a computer

AI-generated content may be incorrect.A screenshot of a computer

AI-generated content may be incorrect.

Sam za ocenjevanje rabmo sprement tole na   
  
A screenshot of a computer

AI-generated content may be incorrect.A screenshot of a computer

AI-generated content may be incorrect.

Kar pomen da **ugasnemo** enp0s3(Vmesnik 1) in nastavimo enp0s8(Vmesnik 2) na **Povezani Vmesnik.**

Kar se tiče nastavitev v VM programu smo konc zaženemo virtualko

A screenshot of a computer

AI-generated content may be incorrect.

1. Nastavlanje cofig nastavitev za omrežje
2. Login

A screenshot of a computer

AI-generated content may be incorrect.

Login: skrbnik

Password: Passw0rd!


1. Pol mormo jit v root način z komando **sudo su**

Ponovno napišemo geslo

1. Pol gremo v config file z komando nano /etc/network/interfaces  
   A screenshot of a computer

   AI-generated content may be incorrect.

In se nm pokaže tole:



File ne bo zgledu tko na začetku ampak ok ni panike sam mormo kopirat to kar je Kralj napisu pod obvestila v moodle -> Povezovanje navideznega stroja na ocenjevanu

A screenshot of a computer

AI-generated content may be incorrect.

1. K je to nastavlen lahko probamo zalaufat apt update in bo vrjetno vrgl vn error : 0% [Working] -> če to vidš klikn ctrl+c
   1. Klič Kralja v večini je problem v /etc/resolv.conf tm rabš spremit iz **nameserver nekip** na **nameserver 8.8.8.8**(googlov dns) al pa **nameserver** **100.64.0.126**(kraljev dns za ocenjevanje)
   2. A screenshot of a computer

      AI-generated content may be incorrect.
2. Zdej rečmo vse dela lahko pingamo 8.8.8.8**(ping 8.8.8.8)**
3. Zdej lahko začnemo z ištalacijo apach2 serverja in openssh-server
   1. Web server – sudo apt install apache2

A black background with white text

AI-generated content may be incorrect.

Potem pritisnemo Y ko nas vpraša če želimo nadaljevati neki tazga

* 1. SSH – sudo apt install openssh-server

A close-up of a black and white sign

AI-generated content may be incorrect.

Zdej mamo vse narjen super! Zdej rabmo sam spletno stran iz NAT-a spravt pa smo!

1. Port Forwarding

Gremo nazaj v control panel od routerja torej na 192.168.1.1

Tm poiščemo gumb Port Mapping spodaj desno

A screenshot of a phone

AI-generated content may be incorrect.

Odbre se nm tole

A screenshot of a computer

AI-generated content may be incorrect. in kliknemo **New**

A screenshot of a computer

AI-generated content may be incorrect.

Se nm odpre tole:

A screenshot of a computer

AI-generated content may be incorrect.

napiše tole not za HTTP port Mapping in Address v okvirčku  **To Address** napišeš ip iz vrstice k piše address (/etc/network/interfaces)A screenshot of a computer screen

AI-generated content may be incorrect.

Ponoviš za SSH

A screenshot of a computer

AI-generated content may be incorrect.

To je to naprej je pa sam z nastavlanje domene in je straight forward

Morm dopisat V1.0

Jon PA